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Abstract:

An overview and status of NASA’s Orion Artemis II Optical Communications (O2O) demonstration will be presented. O2O provides up to 250 Mbps optical downlink and 20 Mbps uplink for mission data transfer and real-time video. 
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